
|  |  |
| --- | --- |
| HBC | MKP X2 金属化聚丙烯薄膜抑制电源电磁干扰电容器 |
|  |
| X2 Metallized Polypropylene Film Capacitor-MKP X2 |

**Interference** **Suppression** **Capacitors(Class** **X2,310VAC)**



**FEATURES**

►Non-inductive,(UL940V-0)plastic case sealed with epoxy resin.

►Provides interference suppression with VDE, ENEC and UL approvals.

►Used in across-the-line, interference suppression circuit.

**SPECIFICATIONS**

Operating Temperature Voltage Rating Capacitance Range Capacitance Tolerance

Package

Insulation Resistance

Dissipation Factor

Voltage Proof

**SAFETY** **APPROVALS:**

-40℃~+110℃

275VAC 305VAC 310VAC

0.0047 ～ 10.0μF

±10%(K)standard,

Bulk, Ammo Tape Package

CR≤0.33 μF, I.R≥15,000MΩ

CR>0.33 μF,I.R≥5,000S (20 ℃,100V,1min)

0.0010μF≤CR≤0.47μF≤0.1%(1KHz,20 ℃)

0.47μF≤CR≤1.0μF≤0.2%(1KHz,20 ℃)

1.0μF≤CR≤10μF≤0.3%(1KHz,20 ℃)

4.3UR DC /5s

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **LOGO**  **MARK** | **COUNTRY** | **APPROVAL**  **STANDARD** | **APPROVAL**  **NO.** | **CLASS** | **CAP.**  **RANGE** | **RATED** **VOLTAGE** |
| **VDE** |  | GERMANY | DIN EN 60384-14  (VDE 0565 Teil 1-1) | 40044146 | X2 | 0.0047 to  10.0pF | 310/305/275VAC |
| **ENEC** |  | EUROPE | EN 60384-14;  IEC 60384-14 | 40044146 | X2 | 0.0047 to  10.0μF | 310/305/275VAC |
| **cUL,**  **UL** |  | CANADA/U.S.A | UL/IEC 60384-14 | E484909 | X2 | 0.0047 to  10.0μF | 310/305/275VAC |
| **CQC** |  | CHINA | IEC 60384-14:2013  +AMDI2016 | CQC16001150050 | X2 | 0.0047 to  10.0μF | 310/305/275VAC |
| **KC** |  | South Korea | KC60384-14 | SU03111 | X2 | 0.0047 to  1.0μF | 310/305/275VAC |

**ENEC mark has replaced all the following European National marks:**






|  |  |  |
| --- | --- | --- |
| **Shantou Xin Hua Xiong Electronios Industry Co.,Ltd.** | | |
| **www.cn-huaxiong.com** | **Tel:【+86】0754-87727171** | **QQ:2851010898** |
| **E-mail:133269599@qq.com** | **Fax:【+86】 0754-87728582** | **whatsapp:86+15502000092** |



|  |  |
| --- | --- |
| HBC | MKP X2 金属化聚丙烯薄膜抑制电源电磁干扰电容器 |
|  |
| X2 Metallized Polypropylene Film Capacitor-MKP X2 |

**Interference** **Suppression** **Capacitors(Class** **X2,310VAC)**

**DRAWING:**



**Dimensions** **Table** **for** **310V** **AC:**

(Unit:mm)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Part#** **Bulk** **Package(Loose** **in** **Box)** | | | | | | |
| **CAP** | **L±1.0** | **H±1.0** | **T±1.0** | **P±1.0** | **d Ø±0.05** | **Standard leads 20mm Min** |
| **0.0047** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9472K100000B |
| **0.0047** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9472K100000B01 \* |
| **0.0056** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9562K100000B |
| **0.0056** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9562K100000B01 \* \* |
| **0.0068** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9682K100000B |
| **0.0068** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9682K100000B01 \* |
| **0.0082** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9822K100000B |
| **0.0082** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9822K100000B01 \* |
| **0.01** | 13 | 9 | 4 | 10 | 0.6 | KPOA9103K100000B01 \* |
| **0.01** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9103K100000B \* |
| **0.01** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9103K150000B \* |
| **0.012** | 13 | 9 | 4 | 10 | 0.6 | MKP0A9123K100000B01 |
| **0.012** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9123K100000B \* |
| **0.012** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9123K150000B \* |
| **0.015** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9153K100000B01 |
| **0.015** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9153K100000B \* |
| **0.015** | 18 | 11 | 5 | 15 | 0.8 | MKP0A9153K150000B \* |
| **0.018** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9183K100000B01 |
| **0.018** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9183K100000B \* |
| **0.018** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9183K150000B \* |
| **0.02** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9203K100000B01 |
| **0.02** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9203K100000B \* |
| **0.02** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9203K150000B \* |
| **0.022** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9223K100000B01 |
| **0.022** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9223K100000B |
| **0.022** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9223K150000B |
| **0.027** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9273K100000B01 \* |
| **0.027** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9273K100000B \* |
| **0.027** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9273K150000B |
| **0.033** | 13 | 9 | 4 | 10 | 0.6 | MKPOA9333K100000B01 |
| **0.033** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9333K100000B \* |
| **0.033** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9333K150000B \* |
| **0.033** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9333K150000B01 |
| **0.039** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9393K100000B |
| **0.039** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9393K100000B01 \* |
| **0.039** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9393K150000B \* |
| **0.047** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9473K100000B |
| **0.047** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9473K100000B01 \* |
| **0.047** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9473K150000B \* |
| **0.056** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9563K100000B01 \* |
| **0.056** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9563K100000B |
| **0.056** | 13 | 13 | 7 | 10 | 0.6 | MKP0A9563K100000B02 |
| **0.056** | 13 | 15 | 8 | 10 | 0.6 | MKP0A9563K100000B03 |
| **0.056** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9563K150000B \* |
| **0.068** | 12 | 11 | 5 | 10 | 0.6 | MKPOA9683K100000B01 |

**Remark:“\*”** **stands** **for** **common** **size.**

Please visit our website to get more update data, those data & specification are subject to change without notice.

|  |  |  |
| --- | --- | --- |
| **Shantou Xin Hua Xiong Electronios Industry Co.,Ltd.** | | |
| **www.cn-huaxiong.com** | **Tel:【+86】0754-87727171** | **QQ:2851010898** |
| **E-mail:133269599@qq.com** | **Fax:【+86】 0754-87728582** | **whatsapp:86+15502000092** |



|  |  |
| --- | --- |
| HBC | MKPX2 金属化聚丙烯薄膜抑制电源电磁干扰电容器 |
|  |
| X2 Metallized Polypropylene Film Capacitor-MKP X2 |

**Interference** **Suppression** **Capacitors(Class** **X2,310VAC)**

**Dimensions** **Table** **for** **310V** **AC:**

(Unit:mm)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Part#** **Bulk** **Package(Loose** **in** **Box)** | | | | | | |
| **CAP** | **L±1.0** | **H±1.0** | **T±1.0** | **P±1.0** | **d Ø±0.05** | **Standard leads 20mm Min** |
| **0.068** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9683K100000B \* |
| **0.068** | 13 | 15 | 8 | 10 | 0.6 | MKPOA9683K100000B02 |
| **0.068** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9683K150000B \* |
| **0.082** | 12 | 11 | 5 | 10 | 0.6 | MKPOA9823K100000B01 |
| **0.082** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9823K100000B \* |
| **0.082** | 13 | 13 | 7 | 10 | 0.6 | MKPOA9823K100000B02 |
| **0.082** | 13 | 15 | 8 | 10 | 0.6 | MKPOA9823K100000B03 |
| **0.082** | 18 | 11 | 5 | 15 | 0.8 | MKP0A9823K150000B \* |
| **0.1** | 13 | 11 | 5 | 10 | 0.6 | MKPOA9104K100000B01 \* |
| **0.1** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9104K100000B |
| **0.1** | 13 | 13 | 7 | 10 | 0.6 | MKPOA9104K100000B02 |
| **0.1** | 13 | 15 | 8 | 10 | 0.6 | MKPOA9104K100000B03 |
| **0.1** | 18 | 11 | 5 | 15 | 0.8 | MKPOA9104K150000B01 \* |
| **0.1** | 18 | 12 | 6 | 15 | 0.8 | MKP0A9104K150000B |
| **0.1** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9104K150000B02 |
| **0.1** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9104K150000B03 |
| **0.1** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKP0A9104K225000B \* |
| **0.12** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9124K100000B01 \* |
| **0.12** | 13 | 13 | 7 | 10 | 0.6 | MKPOA9124K100000B |
| **0.12** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9124K150000B \* |
| **0.13** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9134K150000B \* |
| **0.14** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9144K150000B \* |
| **0.15** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9154K100000B \* |
| **0.15** | 13 | 13 | 7 | 10 | 0.6 | MKPOA9154K100000B01 |
| **0.15** | 13 | 14 | 8 | 10 | 0.6 | MKPOA9154K100000B02 |
| **0.15** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9154K150000B \* |
| **0.15** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9154K150000B02 |
| **0.15** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9154K150000B01 |
| **0.15** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9154K225000B \* |
| **0.15** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9154K225000B01 |
| **0.18** | 13 | 13 | 7 | 10 | 0.6 | MKPOA9184K100000B \* |
| **0.18** | 13 | 14 | 8 | 10 | 0.6 | MKPOA9184K100000B01 |
| **0.18** | 13 | 16.5 | 9 | 10 | 0.6 | MKPOA9184K100000B02 |
| **0.18** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9184K150000B01 \* |
| **0.18** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9184K150000B |
| **0.18** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9184K150000B02 |
| **0.18** | 18 | 15.5 | 9.5 | 15 | 0.8 | MKPOA9184K150000B03 |
| **0.18** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9184K225000B \* |
| **0.2** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9204K150000B  \* |
| **0.2** | 18 | 15.5 | 9.5 | 15 | 0.8 | MKPOA9204K150000B01 |
| **0.2** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9204K225000B \* |
| **0.2** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9204K225000B01 |
| **0.22** | 13 | 12 | 6 | 10 | 0.6 | MKPOA9224K100000B \* |
| **0.22** | 13 | 14 | 8 | 10 | 0.6 | MKPOA9224K100000B01 |

**Remark:“\*”** **stands** **for** **common** **size.**

Please visit our website to get more update data, those data & specification are subject to change without notice.





|  |  |  |
| --- | --- | --- |
| **Shantou Xin Hua Xiong Electronios Industry Co.,Ltd.** | | |
| **www.cn-huaxiong.com** | **Tel:【+86】0754-87727171** | **QQ:2851010898** |
| **E-mail:133269599@qq.com** | **Fax:【+86】 0754-87728582** | **whatsapp:86+15502000092** |

|  |  |
| --- | --- |
| HBC | MKP X2 金属化聚丙烯薄膜抑制电源电磁干扰电容器 |
|  |
| X2 Metallized Polypropylene Film Capacitor-MKP X2 |

**Interference** **Suppression** **Capacitors(Class** **X2,310VAC)**

**Dimensions** **Table** **for** **310V** **AC:**

(Unit:mm)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Part#** **Bulk** **Package(Loose** **in** **Box)** | | | | | | |
| **CAP** | **L±1.0** | **H±1.0** | **T±1.0** | **P±1.0** | **d** **Ø±0.05** | **Standard** **leads** **20mm** **Min** |
| **0.22** | 13 | 15 | 8 | 10 | 0.6 | MKPOA9224K100000B02 |
| **0.22** | 13 | 16.5 | 9 | 10 | 0.6 | MKPOA9224K100000B03 |
| **0.22** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9224K150000B \* |
| **0.22** | 18 | 13 | 7 | 15 | 0.8 | MKPOA9224K150000B01 |
| **0.22** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9224K150000B02 |
| **0.22** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9224K150000B03 |
| **0.22** | 18 | 15.5 | 9.5 | 15 | 0.8 | MKPOA9224K150000B04 |
| **0.22** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9224K225000B |
| **0.22** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9224K225000B01 |
| **0.27** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9274K150000B01 \* |
| **0.27** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9274K150000B |
| **0.27** | 18 | 16 | 10 | 15 | 0.8 | MKP0A9274K150000B02 |
| **0.27** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9274K225000B01 \* |
| **0.27** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9274K225000B |
| **0.33** | 18 | 12 | 6 | 15 | 0.8 | MKPOA9334K150000B01 \* |
| **0.33** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9334K150000B02 |
| **0.33** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9334K150000B |
| **0.33** | 18 | 15.5 | 9.5 | 15 | 0.8 | MKPOA9334K150000B03 |
| **0.33** | 18 | 16 | 10 | 15 | 0.8 | MKPOA9334K150000B04 |
| **0.33** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9334K225000B01 \* |
| **0.33** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9334K225000B |
| **0.33** | 26.5 | 17 | 8.5 | 22.5 | 0.8 | MKPOA9334K225000B02 |
| **0.39** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9394K150000B01 \* |
| **0.39** | 18 | 15.5 | 9.5 | 15 | 0.8 | MKPOA9394K150000B03 |
| **0.39** | 18 | 16 | 10 | 15 | 0.8 | MKPOA9394K150000B04 |
| **0.39** | 18 | 16.5 | 8.4 | 15 | 0.8 | MKPOA9394K150000B02 |
| **0.39** | 18 | 19 | 11 | 15 | 0.8 | MKPOA9394K150000B |
| **0.39** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9394K225000B01 \* |
| **0.39** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9394K225000B02 |
| **0.39** | 26.5 | 17 | 8.5 | 22.5 | 0.8 | MKPOA9394K225000B |
| **0.41** | 26.5 | 17 | 8.5 | 22.5 | 0.8 | MKPOA9414K225000B \* |
| **0.47** | 18 | 13.5 | 7.5 | 15 | 0.8 | MKPOA9474K150000B02 |
| **0.47** | 18 | 14.5 | 8.5 | 15 | 0.8 | MKPOA9474K150000B03 \* |
| **0.47** | 18 | 15.5 | 9.5 | 15 | 0.8 | MKPOA9474K150000B |
| **0.47** | 18 | 16 | 10 | 15 | 0.8 | MKPOA9474K150000B01 |
| **0.47** | 18 | 19 | 11 | 15 | 0.8 | MKPOA9474K150000B04 |
| **0.47** | 26 | 21.5 | 12 | 22.5 | 0.8 | MKPOA9474K225000B04 |
| **0.47** | 26.5 | 15 | 6 | 22.5 | 0.8 | MKPOA9474K225000B02 \* |
| **0.47** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9474K225000B01 |
| **0.47** | 26.5 | 17 | 8.5 | 22.5 | 0.8 | MKPOA9474K225000B |
| **0.47** | 26.5 | 19 | 10 | 22.5 | 0.8 | MKP0A9474K225000B03 |
| **0.47** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKPOA9474K275000B \* |
| **0.56** | 18 | 16 | 10 | 15 | 0.8 | MKPOA9564K150000B \* |
| **0.56** | 18 | 19 | 11 | 15 | 0.8 | MKP0A9564K150000B01 |
| **0.56** | 26.5 | 16.5 | 7 | 22.5 | 0.8 | MKPOA9564K225000B01 \* |
| **0.56** | 26.5 | 17 | 8.5 | 22.5 | 0.8 | MKP0A9564K225000B02 |

Remark:“\*” stands for common size.

Please visit our website to get more update data, those data & specification are subject to change without notice.



|  |  |  |
| --- | --- | --- |
| **Shantou Xin Hua Xiong Electronios Industry Co.,Ltd.** | | |
| **www.cn-huaxiong.com** | **Tel:【+86】0754-87727171** | **QQ:2851010898** |
| **E-mail:133269599@qq.com** | **Fax:【+86】 0754-87728582** | **whatsapp:86+15502000092** |



|  |  |
| --- | --- |
| HBC | MKP X2 金属化聚丙烯薄膜抑制电源电磁干扰电容器 |
|  |
| X2 Metallized Polypropylene Film Capacitor-MKP X2 |

**Interference** **Suppression** **Capacitors(Class** **X2,310VAC)**

**Dimensions** **Table** **for** **310V** **AC:**

(Unit:mm)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Part#** **Bulk** **Package(Loose** **in** **Box)** | | | | | | |
| **CAP** | **L±1.0** | **H±1.0** | **T±1.0** | **P±1.0** | **d** **Ø±0.05** | **Standard** **leads** **20mm** **Min** |
| **0.56** | 26.5 | 19 | 10 | 22.5 | 0.8 | MKPOA9564K225000B |
| **0.56** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKPOA9564K275000B \* |
| **0.68** | 18 | 19 | 11 | 15 | 0.8 | MKP0A9684K150000B \* |
| **0.68** | 26.5 | 17 | 8.5 | 22.5 | 0.8 | MKPOA9684K225000B01 \* |
| **0.68** | 26.5 | 19 | 10 | 22.5 | 0.8 | MKP0A9684K225000B |
| **0.68** | 31 | 25 | 14 | 27.5 | 0.8 | MKPOA9684K275000B01 |
| **0.68** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKPOA9684K275000B \* |
| **0.82** | 26 | 21.5 | 12 | 22.5 | 0.8 | MKP0A9824K225000B |
| **0.82** | 26.5 | 19 | 10 | 22.5 | 0.8 | MKPOA9824K225000B01 \* |
| **0.82** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKPOA9824K275000B \* |
| **1.0** | 26 | 20 | 11 | 22.5 | 0.8 | MKPOA9105K225000B02 |
| **1.0** | 26 | 21.5 | 12 | 22.5 | 0.8 | MKPOA9105K225000B |
| **1.0** | 26.5 | 19 | 10 | 22.5 | 0.8 | MKP0A9105K225000B01 \* |
| **1.0** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKP0A9105K275000B \* |
| **1.0** | 31.5 | 21.6 | 13 | 27.5 | 0.8 | MKPOA9105K275000B01 |
| **1.2** | 26 | 20 | 11 | 22.5 | 0.8 | MKPOA9125K225000B01 |
| **1.2** | 26 | 21.5 | 12 | 22.5 | 0.8 | MKPOA9125K225000B02 |
| **1.2** | 26.5 | 19 | 10 | 22.5 | 0.8 | MKP0A9125K225000B \* |
| **1.2** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKPOA9125K275000B01 \* |
| **1.2** | 31.5 | 21.6 | 13 | 27.5 | 0.8 | MKP0A9125K275000B |
| **1.5** | 26 | 21.5 | 12 | 22.5 | 0.8 | MKPOA9155K225000B \* |
| **1.5** | 31 | 25 | 14 | 27.5 | 0.8 | MKPOA9155K275000B02 |
| **1.5** | 31.5 | 19.5 | 10.8 | 27.5 | 0.8 | MKP0A9155K275000B01 \* |
| **1.5** | 31.5 | 21.6 | 13 | 27.5 | 0.8 | MKPOA9155K275000B |
| **1.8** | 31 | 25 | 14 | 27.5 | 0.8 | MKP0A9185K275000B |
| **1.8** | 31.5 | 21.6 | 13 | 27.5 | 0.8 | MKPOA9185K275000B01 \* |
| **2.2** | 31 | 25 | 14 | 27.5 | 0.8 | MKPOA9225K275000B \* |
| **2.2** | 32 | 25.5 | 16 | 27.5 | 0.8 | MKPOA9225K275000B01 |
| **\*2.2** | 32 | 28 | 18 | 27.5 | 0.8 | MKPOA9225K275000B02 |
| **\*2.2** | 42 | 28 | 14 | 37.5 | 0.8 | MKP0A9225K375000B \* |
| **2.7** | 31 | 25 | 14 | 27.5 | 0.8 | MKP0A9275K275000B01 |
| **2.7** | 32 | 25.5 | 16 | 27.5 | 0.8 | MKP0A9275K275000B02 \* |
| **2.7** | 32 | 28 | 18 | 27.5 | 0.8 | MKP0A9275K275000B |
| **2.7** | 42 | 28 | 14 | 37.5 | 0.8 | MKP0A9275K375000B \* |
| **2.8** | 32 | 25.5 | 16 | 27.5 | 0.8 | MKP0A9285K275000B \* |
| **3.3** | 32 | 28 | 18 | 27.5 | 0.8 | MKP0A9335K275000B \* |
| **3.3** | 41 | 32 | 17 | 37.5 | 0.8 | MKP0A9335K375000B \* |
| **3.9** | 41 | 32 | 17 | 37.5 | 0.8 | MKP0A9395K375000B \* |
| **4.7** | 32 | 37 | 22 | 27.5 | 0.8 | MKP0A9475K275000B \* |
| **4.7** | 41 | 33.5 | 18.5 | 37.5 | 0.8 | MKP0A9475K375000B \* |
| **5.6** | 41 | 37 | 22 | 37.5 | 0.8 | MKP0A9565K375000B \* |
| **6.8** | 41 | 37 | 22 | 37.5 | 0.8 | MKP0A9685K375000B \* |
| **8.2** | 41 | 41 | 26 | 37.5 | 0.8 | MKP0A9825K375000B \* |
| **10.0** | 41 | 43 | 28 | 37.5 | 0.8 | MKP0A9106K375000B \* |

**Remark;“\*”** **stands** **for** **common** **size.**

Please visit our website to get more update data, those data & specification are subject to change without notice.



|  |  |  |
| --- | --- | --- |
| **Shantou Xin Hua Xiong Electronios Industry Co.,Ltd.** | | |
| **www.cn-huaxiong.com** | **Tel:【+86】0754-87727171** | **QQ:2851010898** |
| **E-mail:133269599@qq.com** | **Fax:【+86】 0754-87728582** | **whatsapp:86+15502000092** |

